# Static Call Graph for image .\Objects\project.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Wed Aug 21 10:23:31 2024

### Maximum Stack Usage = 120 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ wifi_rx_Control ⇒ OLED_SHOW ⇒ OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_DrawPoint

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - ADC3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - BusFault_Handler from stm32f10x_it.o(i.BusFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA1_Channel7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DMA2_Channel4_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - DebugMon_Handler from stm32f10x_it.o(i.DebugMon_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI15_10_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - EXTI9_5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FLASH_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - FSMC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - HardFault_Handler from stm32f10x_it.o(i.HardFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - MemManage_Handler from stm32f10x_it.o(i.MemManage_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - NMI_Handler from stm32f10x_it.o(i.NMI_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - PVD_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - PendSV_Handler from stm32f10x_it.o(i.PendSV_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - RCC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTCAlarm_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - RTC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - Reset_Handler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SDIO_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI1_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SPI3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - SVC_Handler from stm32f10x_it.o(i.SVC_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SysTick_Handler from stm32f10x_it.o(i.SysTick_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - SystemInit from system_stm32f10x.o(i.SystemInit) referenced from startup_stm32f10x_hd.o(.text)
  - TAMPER_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM6_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM7_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_BRK_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_CC_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_TRG_COM_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - TIM8_UP_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART4_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UART5_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART1_IRQHandler from usart.o(i.USART1_IRQHandler) referenced from startup_stm32f10x_hd.o(RESET)
  - USART2_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USART3_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - UsageFault_Handler from stm32f10x_it.o(i.UsageFault_Handler) referenced from startup_stm32f10x_hd.o(RESET)
  - WWDG_IRQHandler from startup_stm32f10x_hd.o(.text) referenced from startup_stm32f10x_hd.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f10x_hd.o(.text)
  - _sputc from printf2.o(i._sputc) referenced from printf2.o(i.__0sprintf$2)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  ADC3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  DMA2_Channel4_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  FSMC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTCAlarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SDIO_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SPI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM6_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM7_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  TIM8_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  UART5_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f10x_hd.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text))
  [Calls]

  - >> __aeabi_memset
  [Called By]
  - >> WIFI_BUFF_MEMSET

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strstr (Thumb, 36 bytes, Stack size 12 bytes, strstr.o(.text))
  [Stack]

  - Max Depth = 12
  - Call Chain = strstr
  [Called By]
  - >> wifi_rx_Control
  - >> WIFI_CheckAck

  strlen (Thumb, 14 bytes, Stack size 0 bytes, strlen.o(.text))
  [Called By]

  - >> wifi_rx_Control
  - >> WIFI_SEND

  strrchr (Thumb, 22 bytes, Stack size 0 bytes, strrchr.o(.text))
  [Called By]

  - >> wifi_rx_Control

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  BusFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.BusFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  CONNECT_TO_UDP (Thumb, 182 bytes, Stack size 64 bytes, wifi.o(i.CONNECT_TO_UDP))
  [Stack]

  - Max Depth = 120
  - Call Chain = CONNECT_TO_UDP ⇒ WIFI_CheckAck ⇒ WIFI_SEND ⇒ USART1_SEND
  [Calls]
  - >> __2sprintf
  - >> WIFI_SEND
  - >> WIFI_CheckAck
  [Called By]
  - >> main

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  GPIO_Config (Thumb, 42 bytes, Stack size 8 bytes, led.o(i.GPIO_Config))
  [Stack]

  - Max Depth = 32
  - Call Chain = GPIO_Config ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  GPIO_Init (Thumb, 278 bytes, Stack size 24 bytes, stm32f10x_gpio.o(i.GPIO_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = GPIO_Init
  [Called By]
  - >> USART2_Config
  - >> USART1_Config
  - >> OLED_Init
  - >> Motor_Config
  - >> GPIO_Config

  GPIO_PinRemapConfig (Thumb, 138 bytes, Stack size 20 bytes, stm32f10x_gpio.o(i.GPIO_PinRemapConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = GPIO_PinRemapConfig
  [Called By]
  - >> OLED_Init

  GPIO_ResetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_ResetBits))
  [Called By]

  - >> wifi_rx_Control
  - >> OLED_Init
  - >> OLED_WR_Byte
  - >> Motor_Control3
  - >> Motor_Control2
  - >> Motor_Control1

  GPIO_SetBits (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_gpio.o(i.GPIO_SetBits))
  [Called By]

  - >> wifi_rx_Control
  - >> OLED_Init
  - >> OLED_WR_Byte
  - >> Motor_Control2
  - >> Motor_Control1

  HardFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.HardFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  MemManage_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.MemManage_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  Motor_Config (Thumb, 42 bytes, Stack size 8 bytes, motor.o(i.Motor_Config))
  [Stack]

  - Max Depth = 32
  - Call Chain = Motor_Config ⇒ GPIO_Init
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  [Called By]
  - >> main

  Motor_Control1 (Thumb, 20 bytes, Stack size 8 bytes, motor.o(i.Motor_Control1))
  [Stack]

  - Max Depth = 8
  - Call Chain = Motor_Control1
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> wifi_rx_Control

  Motor_Control2 (Thumb, 20 bytes, Stack size 8 bytes, motor.o(i.Motor_Control2))
  [Stack]

  - Max Depth = 8
  - Call Chain = Motor_Control2
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> wifi_rx_Control

  Motor_Control3 (Thumb, 20 bytes, Stack size 8 bytes, motor.o(i.Motor_Control3))
  [Stack]

  - Max Depth = 8
  - Call Chain = Motor_Control3
  [Calls]
  - >> GPIO_ResetBits
  [Called By]
  - >> wifi_rx_Control

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.NMI_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  NVIC_Init (Thumb, 100 bytes, Stack size 16 bytes, misc.o(i.NVIC_Init))
  [Stack]

  - Max Depth = 16
  - Call Chain = NVIC_Init
  [Called By]
  - >> USART1_Config

  NVIC_PriorityGroupConfig (Thumb, 10 bytes, Stack size 0 bytes, misc.o(i.NVIC_PriorityGroupConfig))
  [Called By]

  - >> main

  OLED_Clear (Thumb, 42 bytes, Stack size 16 bytes, oled.o(i.OLED_Clear))
  [Stack]

  - Max Depth = 48
  - Call Chain = OLED_Clear ⇒ OLED_Refresh ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_Refresh
  [Called By]
  - >> wifi_rx_Control
  - >> OLED_Init

  OLED_ColorTurn (Thumb, 28 bytes, Stack size 8 bytes, oled.o(i.OLED_ColorTurn))
  [Stack]

  - Max Depth = 24
  - Call Chain = OLED_ColorTurn ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> main

  OLED_DisplayTurn (Thumb, 44 bytes, Stack size 8 bytes, oled.o(i.OLED_DisplayTurn))
  [Stack]

  - Max Depth = 24
  - Call Chain = OLED_DisplayTurn ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> main

  OLED_DrawPoint (Thumb, 114 bytes, Stack size 20 bytes, oled.o(i.OLED_DrawPoint))
  [Stack]

  - Max Depth = 20
  - Call Chain = OLED_DrawPoint
  [Called By]
  - >> OLED_ShowChar
  - >> OLED_ShowChinese

  OLED_Init (Thumb, 308 bytes, Stack size 8 bytes, oled.o(i.OLED_Init))
  [Stack]

  - Max Depth = 56
  - Call Chain = OLED_Init ⇒ OLED_Clear ⇒ OLED_Refresh ⇒ OLED_WR_Byte
  [Calls]
  - >> delay_ms
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> GPIO_PinRemapConfig
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> OLED_WR_Byte
  - >> OLED_Clear
  [Called By]
  - >> main

  OLED_Refresh (Thumb, 70 bytes, Stack size 16 bytes, oled.o(i.OLED_Refresh))
  [Stack]

  - Max Depth = 32
  - Call Chain = OLED_Refresh ⇒ OLED_WR_Byte
  [Calls]
  - >> OLED_WR_Byte
  [Called By]
  - >> OLED_Clear
  - >> OLED_SHOW

  OLED_SHOW (Thumb, 120 bytes, Stack size 8 bytes, wifi.o(i.OLED_SHOW))
  [Stack]

  - Max Depth = 104
  - Call Chain = OLED_SHOW ⇒ OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_DrawPoint
  [Calls]
  - >> OLED_ShowString
  - >> OLED_ShowChinese
  - >> OLED_Refresh
  [Called By]
  - >> wifi_rx_Control

  OLED_ShowChar (Thumb, 300 bytes, Stack size 48 bytes, oled.o(i.OLED_ShowChar))
  [Stack]

  - Max Depth = 68
  - Call Chain = OLED_ShowChar ⇒ OLED_DrawPoint
  [Calls]
  - >> OLED_DrawPoint
  [Called By]
  - >> OLED_ShowString

  OLED_ShowChinese (Thumb, 186 bytes, Stack size 44 bytes, oled.o(i.OLED_ShowChinese))
  [Stack]

  - Max Depth = 64
  - Call Chain = OLED_ShowChinese ⇒ OLED_DrawPoint
  [Calls]
  - >> OLED_DrawPoint
  [Called By]
  - >> OLED_SHOW

  OLED_ShowString (Thumb, 74 bytes, Stack size 28 bytes, oled.o(i.OLED_ShowString))
  [Stack]

  - Max Depth = 96
  - Call Chain = OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_DrawPoint
  [Calls]
  - >> OLED_ShowChar
  [Called By]
  - >> OLED_SHOW

  OLED_WR_Byte (Thumb, 116 bytes, Stack size 16 bytes, oled.o(i.OLED_WR_Byte))
  [Stack]

  - Max Depth = 16
  - Call Chain = OLED_WR_Byte
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  [Called By]
  - >> OLED_Init
  - >> OLED_DisplayTurn
  - >> OLED_ColorTurn
  - >> OLED_Refresh

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  RCC_APB1PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB1PeriphClockCmd))
  [Called By]

  - >> USART2_Config

  RCC_APB2PeriphClockCmd (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_rcc.o(i.RCC_APB2PeriphClockCmd))
  [Called By]

  - >> USART2_Config
  - >> USART1_Config
  - >> OLED_Init
  - >> Motor_Config
  - >> GPIO_Config

  RCC_GetClocksFreq (Thumb, 192 bytes, Stack size 12 bytes, stm32f10x_rcc.o(i.RCC_GetClocksFreq))
  [Stack]

  - Max Depth = 12
  - Call Chain = RCC_GetClocksFreq
  [Called By]
  - >> USART_Init

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SysTick_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f10x_it.o(i.SysTick_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  SystemInit (Thumb, 78 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SystemInit))
  [Stack]

  - Max Depth = 28
  - Call Chain = SystemInit ⇒ SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClock
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(.text)

  USART1_Config (Thumb, 174 bytes, Stack size 32 bytes, usart.o(i.USART1_Config))
  [Stack]

  - Max Depth = 100
  - Call Chain = USART1_Config ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> NVIC_Init
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> USART_Init
  - >> USART_ITConfig
  - >> USART_Cmd
  [Called By]
  - >> main

  USART1_IRQHandler (Thumb, 82 bytes, Stack size 8 bytes, usart.o(i.USART1_IRQHandler))
  [Stack]

  - Max Depth = 24
  - Call Chain = USART1_IRQHandler ⇒ USART_GetITStatus
  [Calls]
  - >> USART_ReceiveData
  - >> USART_GetITStatus
  - >> USART_GetFlagStatus
  - >> USART_ClearITPendingBit
  [Address Reference Count : 1]
  - startup_stm32f10x_hd.o(RESET)

  USART1_SEND (Thumb, 42 bytes, Stack size 16 bytes, usart.o(i.USART1_SEND))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART1_SEND
  [Calls]
  - >> USART_SendData
  - >> USART_GetFlagStatus
  [Called By]
  - >> WIFI_SEND

  USART2_Config (Thumb, 114 bytes, Stack size 32 bytes, usart.o(i.USART2_Config))
  [Stack]

  - Max Depth = 100
  - Call Chain = USART2_Config ⇒ USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> GPIO_Init
  - >> RCC_APB2PeriphClockCmd
  - >> RCC_APB1PeriphClockCmd
  - >> USART_Init
  - >> USART_Cmd
  [Called By]
  - >> main

  USART_ClearITPendingBit (Thumb, 30 bytes, Stack size 8 bytes, stm32f10x_usart.o(i.USART_ClearITPendingBit))
  [Stack]

  - Max Depth = 8
  - Call Chain = USART_ClearITPendingBit
  [Called By]
  - >> USART1_IRQHandler

  USART_Cmd (Thumb, 24 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_Cmd))
  [Called By]

  - >> USART2_Config
  - >> USART1_Config

  USART_GetFlagStatus (Thumb, 26 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_GetFlagStatus))
  [Called By]

  - >> USART1_SEND
  - >> USART1_IRQHandler

  USART_GetITStatus (Thumb, 84 bytes, Stack size 16 bytes, stm32f10x_usart.o(i.USART_GetITStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = USART_GetITStatus
  [Called By]
  - >> USART1_IRQHandler

  USART_ITConfig (Thumb, 74 bytes, Stack size 20 bytes, stm32f10x_usart.o(i.USART_ITConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = USART_ITConfig
  [Called By]
  - >> USART1_Config

  USART_Init (Thumb, 210 bytes, Stack size 56 bytes, stm32f10x_usart.o(i.USART_Init))
  [Stack]

  - Max Depth = 68
  - Call Chain = USART_Init ⇒ RCC_GetClocksFreq
  [Calls]
  - >> RCC_GetClocksFreq
  [Called By]
  - >> USART2_Config
  - >> USART1_Config

  USART_ReceiveData (Thumb, 10 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_ReceiveData))
  [Called By]

  - >> USART1_IRQHandler

  USART_SendData (Thumb, 8 bytes, Stack size 0 bytes, stm32f10x_usart.o(i.USART_SendData))
  [Called By]

  - >> USART1_SEND

  UsageFault_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f10x_it.o(i.UsageFault_Handler))
  [Address Reference Count : 1]

  - startup_stm32f10x_hd.o(RESET)

  WIFI_BUFF_MEMSET (Thumb, 26 bytes, Stack size 8 bytes, wifi.o(i.WIFI_BUFF_MEMSET))
  [Stack]

  - Max Depth = 8
  - Call Chain = WIFI_BUFF_MEMSET
  [Calls]
  - >> __aeabi_memclr
  [Called By]
  - >> wifi_rx_Control
  - >> WIFI_CheckAck

  WIFI_CheckAck (Thumb, 74 bytes, Stack size 24 bytes, wifi.o(i.WIFI_CheckAck))
  [Stack]

  - Max Depth = 56
  - Call Chain = WIFI_CheckAck ⇒ WIFI_SEND ⇒ USART1_SEND
  [Calls]
  - >> delay_ms
  - >> strstr
  - >> WIFI_SEND
  - >> WIFI_BUFF_MEMSET
  [Called By]
  - >> CONNECT_TO_UDP

  WIFI_SEND (Thumb, 22 bytes, Stack size 16 bytes, wifi.o(i.WIFI_SEND))
  [Stack]

  - Max Depth = 32
  - Call Chain = WIFI_SEND ⇒ USART1_SEND
  [Calls]
  - >> strlen
  - >> USART1_SEND
  [Called By]
  - >> CONNECT_TO_UDP
  - >> WIFI_CheckAck

  __0sprintf$2 (Thumb, 34 bytes, Stack size 24 bytes, printf2.o(i.__0sprintf$2), UNUSED)
  [Calls]

  - >> _sputc
  - >> _printf_core

  __1sprintf$2 (Thumb, 0 bytes, Stack size 24 bytes, printf2.o(i.__0sprintf$2), UNUSED)

  __2sprintf (Thumb, 0 bytes, Stack size 24 bytes, printf2.o(i.__0sprintf$2))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2sprintf
  [Called By]
  - >> CONNECT_TO_UDP

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  delay_ms (Thumb, 20 bytes, Stack size 8 bytes, delay.o(i.delay_ms))
  [Stack]

  - Max Depth = 8
  - Call Chain = delay_ms
  [Calls]
  - >> delay_us
  [Called By]
  - >> OLED_Init
  - >> WIFI_CheckAck

  delay_us (Thumb, 158 bytes, Stack size 0 bytes, delay.o(i.delay_us))
  [Called By]

  - >> delay_ms

  main (Thumb, 82 bytes, Stack size 0 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 120
  - Call Chain = main ⇒ wifi_rx_Control ⇒ OLED_SHOW ⇒ OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_DrawPoint
  [Calls]
  - >> wifi_rx_Control
  - >> USART2_Config
  - >> USART1_Config
  - >> OLED_Init
  - >> OLED_DisplayTurn
  - >> OLED_ColorTurn
  - >> NVIC_PriorityGroupConfig
  - >> Motor_Config
  - >> GPIO_Config
  - >> CONNECT_TO_UDP
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  wifi_rx_Control (Thumb, 250 bytes, Stack size 16 bytes, wifi.o(i.wifi_rx_Control))
  [Stack]

  - Max Depth = 120
  - Call Chain = wifi_rx_Control ⇒ OLED_SHOW ⇒ OLED_ShowString ⇒ OLED_ShowChar ⇒ OLED_DrawPoint
  [Calls]
  - >> GPIO_SetBits
  - >> GPIO_ResetBits
  - >> strrchr
  - >> strlen
  - >> strstr
  - >> OLED_Clear
  - >> Motor_Control3
  - >> Motor_Control2
  - >> Motor_Control1
  - >> WIFI_BUFF_MEMSET
  - >> OLED_SHOW
  [Called By]
  - >> main

  ### Local Symbols

  SetSysClock (Thumb, 8 bytes, Stack size 8 bytes, system_stm32f10x.o(i.SetSysClock))
  [Stack]

  - Max Depth = 20
  - Call Chain = SetSysClock ⇒ SetSysClockTo72
  [Calls]
  - >> SetSysClockTo72
  [Called By]
  - >> SystemInit

  SetSysClockTo72 (Thumb, 214 bytes, Stack size 12 bytes, system_stm32f10x.o(i.SetSysClockTo72))
  [Stack]

  - Max Depth = 12
  - Call Chain = SetSysClockTo72
  [Called By]
  - >> SetSysClock

  _printf_core (Thumb, 214 bytes, Stack size 40 bytes, printf2.o(i._printf_core), UNUSED)
  [Called By]

  - >> __0sprintf$2

  _sputc (Thumb, 10 bytes, Stack size 0 bytes, printf2.o(i._sputc))
  [Called By]

  - >> __0sprintf$2
  [Address Reference Count : 1]
  - printf2.o(i.__0sprintf$2)

  ### Undefined Global Symbols